PLEASE NOTE: The Office of the Revisor of Statutes cannot perform research, provide legal advice, or interpret Maine law. For legal assistance, please contact a qualified attorney.
Public Law
124th Legislature
First Regular Session
Chapter 250
H.P. 46 - L.D. 53
An Act To Permit the Use of a Common Flue for Oil and Solid Fuel Burning Equipment
Be it enacted by the People of the State of Maine as follows:
Sec. 1.   25 MRSA §2465, sub-§1-A,  as enacted by PL 2005, c. 571, §1, is amended to read:
 
1-A. Routine technical rules.    The Commissioner of Public Safety shall adopt rules pertaining to the construction, installation, maintenance and inspection of chimneys, fireplaces, vents and solid fuel burning appliances. Rules adopted pursuant to this subsection may include rules pertaining to maintenance and inspections, except as provided in subsection 1-B. Rules adopted pursuant to this subsection may not prohibit the continued use of an existing connection of a solid fuel burning appliance to a chimney flue to which another appliance burning oil or solid fuel is connected for any chimney existing and in use prior to February 2, 1998 as long as sufficient draft is available for each appliance, the chimney is lined and structurally intact and a carbon monoxide detector is installed in the building near a bedroom. Rules adopted pursuant to this subsection are routine technical rules as defined in Title 5, chapter 375, subchapter 2-A.
Sec. 2.   32 MRSA §2402-A,  as enacted by PL 1999, c. 386, Pt. J, §16, is amended to read:
§ 2402-A.  Rules
The board may adopt reasonable rules for the issuance of various types and classes of licenses to cover oil and solid fuel burner installations and to set forth standards and rules for product approval. Rules adopted pursuant to this section may not prohibit the continued use of an existing connection of a solid fuel burning appliance to a chimney flue to which another appliance burning oil or solid fuel is connected for any chimney existing and in use prior to February 2, 1998 as long as sufficient draft is available for each appliance, the chimney is lined and structurally intact and a carbon monoxide detector is installed in the building near a bedroom. A license may cover one or more types of installations. The board may further adopt reasonable rules concerning the term and type of experience required by candidates for examination.
 
Effective September 12, 2009