PLEASE NOTE: The Office of the Revisor of Statutes cannot perform research, provide legal advice, or interpret Maine law. For legal assistance, please contact a qualified attorney.
Public Law
124th Legislature
Second Regular Session
Chapter 535
S.P. 681 - L.D. 1775
An Act To Amend Mercury Stack Testing Requirements for Certain Air Emission Sources
Be it enacted by the People of the State of Maine as follows:
Sec. 1.   38 MRSA §585-B, sub-§5,  as amended by PL 2009, c. 338, §1, is further amended to read:
 
5. Standards for mercury.    Notwithstanding subsection 1, an air emission source may not emit mercury in excess of 45.4 kilograms, or 100 pounds, per year after January 1, 2000; 22.7 kilograms, or 50 pounds, per year after January 1, 2004; 15.9 kilograms, or 35 pounds, after January 1, 2007; and 11.4 kilograms, or 25 pounds, after January 1, 2010. As an alternative to not emitting mercury in excess of 11.4 kilograms, or 25 pounds, after January 1, 2010, an air emission source may reduce mercury emissions by 90 percent by weight after January 1, 2010. Compliance with these limits must be specified in the license of the air emission source. The board shall establish by rule testing protocols and measurement methods for emissions sources for which the board has not established such protocols and methods for determining compliance with the emission standard for mercury. These rules are routine technical rules under Title 5, chapter 375, subchapter 2-A.
 
An air emission source may apply to the board for an extension or modification of the 11.4-kilogram, or 25-pound, limit as follows.
 
A. An emission source may submit an application to the board no later than January 1, 2009 for a 6-month extension of the January 1, 2010 deadline to meet the 11.4-kilogram, or 25-pound, limit. The board shall grant the extension if the board determines, based on information presented by the source, that compliance with the limit is not achievable by the deadline due to engineering constraints, availability of equipment or other justifiable technical reasons.
 
B. An emission source may submit an application to the board no later than January 1, 2009 for a license modification establishing an alternative emission limit for mercury. The board shall grant the license modification if the board finds that the proposed mercury emission limit meets the most stringent emission limitation that is achievable and compatible with that class of source, considering economic feasibility.
 
Pending a decision on an application for an extension or a license modification under this subsection, the 15.9-kilogram, or 35-pound, limit applies to the emission source.
 
Notwithstanding the January 1, 2000 compliance date in this subsection, a resource recovery facility that is subject to an emissions limit for mercury adopted by rule by the board before January 1, 2000 shall comply with the 45.4-kilogram, or 100-pound, mercury emissions limit after December 19, 2000.
 
For determining compliance with this subsection, the results of multiple stack tests may be averaged in accordance with guidance provided by the department.
Sec. 2.   38 MRSA §585-B, sub-§6,  as amended by PL 2009, c. 338, §2, is further amended to read:
 
6. Mercury reduction plans.    Any An air emission source emitting mercury in excess of 10 pounds per year after January 1, 2007 must develop a mercury reduction plan. The Except as provided in subsection 7, the mercury reduction plan must be submitted to the department no later than September 1, 2008. The mercury reduction plan must contain:
 
A. Identification, characterization and accounting of the mercury used or released at the emission source; and
 
B. Identification, analysis and evaluation of any appropriate technologies, procedures, processes, equipment or production changes that may be utilized by the emission source to reduce the amount of mercury used or released by that emission source, including a financial analysis of the costs and benefits of reducing the amount of mercury used or released.
 
The department may keep information submitted to the department under this subsection confidential as provided under section 1310-B.
 
The department shall submit a report to the joint standing committee of the Legislature having jurisdiction over natural resources matters no later than March 1, 2009 summarizing the mercury emissions and mercury reduction potential from those emission sources subject to this subsection. In addition, the department shall include an evaluation of the appropriateness of the 25-pound mercury standard established in subsection 5. The evaluation must address, but is not limited to, the technological feasibility, cost and schedule of achieving the standards established in subsection 5. The department shall submit an updated report to the committee by January 1, 2010 March 1, 2013. The joint standing committee of the Legislature having jurisdiction over natural resources matters is authorized to report out to the 124th 126th Legislature legislation a bill relating to the evaluation and the updated report.
Sec. 3.   38 MRSA §585-B, sub-§7  is enacted to read:
 
7.  Stack tests for mercury.      An air emission source emitting mercury in excess of 10 pounds in calendar year 2010 must:
 
 A.  Conduct a stack test for mercury twice in calendar year 2011 and twice in calendar year 2012. The stack tests must be conducted at least 4 months apart; and
 
 B.  By January 1, 2013, develop a mercury reduction plan and submit the plan to the department in accordance with subsection 6. The plan must contain the results of the 4 stack tests conducted pursuant to paragraph A.
 
For determining compliance with subsection 5, the results of multiple stack tests under this subsection may be averaged in accordance with guidance provided by the department.
 
The department may approve an alternative to the stack testing requirements in this subsection, such as, but not limited to, mercury input data or a continuous mercury emission monitoring system.
 
Effective July 12, 2010